8000 STOCK TURBO 4X4 CLASS 2025
100% OEM stock charger.
 No rear blocks, no hanging or hidden weight, 
No trick hitches, Reese style hitches only, must pull from rear of truck
Must be able to tow a trailer with the hitch.
Truck must be licensed, insured and street driven.
 Single ladder bar allowed.
No hood stacks, exhaust must exit behind the cab
 If adding weight no more then 8000 lbs, that includes tool boxes and fuel tanks… if have nothing adding weight to truck we allow whatever the truck weights…
20”  Hitch
Hitch must have minimum opening of 3 x 3 ¾, if clevis is used it must be bolted with minimum 1 inch bolt.  No twist clevises allowed.
Engine and turbo must have been available from the factory and been an option in the year/make of truck being pulled.    
Must have 4 working wheel brakes

6500 Street Stock Gas 4x4 2025 
Must be licensed, insured and street driven 
No rear end blocks( Rear of truck cannot be blocked solid, must have minimum 2 inches of possible travel)
No hidden or hanging weight, added weight must be in the bed. 
Must be able to tow a trailer with the hitch
No trick hitches, Reese style hitch only, must pull from rear of truck,  hitch must accept any off the shelf Reese style receiver. 
Single ladder bar allowed 
If adding weight,  No more than 6500 lbs, that includes fuel tanks and tool boxes. If have nothing added to the truck for wieght,  may pull truck at whatever it wieghs..
20 inch hitch
Hitch must have minimum opening of 3 x 3 ¾, if clevis is used it must be bolted with minimum 1 inch bolt.  No twist clevises allowed.
Cast off the shelf intake, max 4150 carb
Aluminum intakes allowed(off the shelf)
Oem block and heads
If truck is fuel Injected, must be the factory efi and look 100 percent stock
1 ton drive line or less
Must have full exhaust and exit behind the cab with mufflers
Maximum of 3” collector and exhaust 
Must have 4 working wheel brakes


